CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Wed Jun 26 07:50:23 2024
Release      : TopSpin 4.3.0
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.3.180.20230524
CPU          : Intel(R) Core(TM) i5-8400H CPU @ 2.50GHz (8 cores at 3612 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 600 NMR spectrometer
1H-frequency : 600.13 MHz
Description  : Avance
Bruker Order : 429128
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- SCU: AV4I SCU SYSTEM CONTROL UNIT Z162978/00403 ECL 02.00
- {EPU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00403 ECL 02.00
- {GTU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00403 ECL 02.00
  Location: slot 7 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312125813
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd2, RTD at /dev/bbu/rtd4.4, GPROC at /dev/bbu/gproc4.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/05988 ECL 02.03
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd11, DRX at /dev/bbu/drx9.5, RTD at /dev/bbu/rtd9.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/05989 ECL 02.03
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.46 via PCIe #11
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx11.5, RTD at /dev/bbu/rtd11.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/05990 ECL 02.03
  Location: slot 5 in rack 1
  Connection: at IP 192.168.180.54 via PCIe #13
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd29, DRX at /dev/bbu/drx13.5, RTD at /dev/bbu/rtd13.4
  Sequencer: FCube
  - FCube3
- PSM-A: AV4 PSM-A Z149510/02402 ECL 03.01
- HPPR/2 COVER2: HPPR/2 Cover2N Z178831/00060 ECL 00.00
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (reflection meter with CRP-Bias capability)
                  PN=Z103205, SN=01388 from 20201218
      Module  2 : 2H
                  PN=Z003473, SN=02036 from 20201201
      Module  3 : XBB19F 2HP
                  PN=Z105186, SN=00583 from 20210115
      Module  4 : 13C/79Br
                  PN=Z003524, SN=01393 from 20201119
      Module  5 : 15N
                  PN=Z003530, SN=01258 from 20201126
  
- HPLNA 1H19F: HPLNA 1H MODULE 600 Z103205/01388 ECL 06.04
- 2H: HPPR/2 2H MODULE 600 Z003473/02036 ECL 07.00
- XBB19F 2HP: HPPR/2 XBB19F 2HP MODULE 600 Z105186/00583 ECL 07.01
- 13C/79Br: HPPR/2 13C MODULE 600 Z003524/01393 ECL 08.00
- 15N: HPPR/2 15N MODULE 600 Z003530/01258 ECL 07.01
- RACK: AV4I AQS CHASSIS Z175600/00273 ECL 00.00
- FANTRAY: AV4I AQS FAN TRAY Z175900/00268 ECL 00.00
- PSM-48V: AV4 PSM-48V Z149850/04102 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/02445 ECL 01.01
- REF 1200: AV4 REFERENCE 1200 Z148270/02088 ECL 02.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144059-000514 W144059/000514 ECL 11:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB500 15-600: W144059/000514 ECL 11
- Controller     = BLA CONTROL BOARD 7: W133936/023417 ECL 40
BLA-W144061-000979 W144061/000979 ECL 22:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABBH500/100 200-600: W144061/000979 ECL 22
- Controller     = BLA CONTROL BOARD 7: W133936/023348 ECL 40
LTRX Z109890/01466 ECL 03.02:
- TCP/IP address = 192.168.99.10
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01466 ECL 03.02

BSMS: BSMS/2 functionality available
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20220429
- ELCB = BSMS/2 ELCB: Z100818/08957 ECL 07.03
- Backplane = AV4 BSMS CHASSIS: Z152144/01396 ECL 03.00
- Fan tray = AV4 BSMS FAN TRAY: Z152145/01716 ECL 00.02
- Power Supply = AV4 BSMS PSM-B POWER SUPPLY: Z150090/01665 ECL 01.01
- Power Supply 48V 1 = AV4 PSM-48V: Z149850/04103 ECL 01.02
- Variable Power Supply 1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/01924 ECL 01.02
- Power Control = AV4 BSMS POWER CONTROL BOARD: Z150089/01739 ECL 01.00
- SLCB functionality: Available
- GAB Z-Gradient = AV4 GAB/2 GRADIENT AMPL BD: Z155150/01932 ECL 00.01
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS3-SB
- SCB channels = 40
- SCB1 = BSMS/2 SCB20: Z102930/13999 ECL 05.00
- SCB2 = BSMS/2 SCB20: Z102930/13969 ECL 05.00
- Shim matrix file: 292722ca.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 Z7 Z8 XZ5 YZ5 (X2-Y2)Z3 (X2-Y2)Z4 (X2-Y2)Z5 XYZ3 XYZ4 XYZ5
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/01466 ECL 03.02
- Lock: On L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/06069 ECL 05.05
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC: Z139305/01924 ECL 01.02
- SampleMail = SM SAMPLEMAIL PLUS 610 KPL.: Z133067/3107 ECL 0.10

SampleCase: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10
-  = SM SAMPLEMAIL PLUS 610 KPL.: Z133067/3107 ECL 0.10
- VTC active channel 1 = BSMS/2 VTA CRP: Z116923/02151 ECL 02.03
- VTC active channel 2 = BSMS/2 VTA SACA: Z141200/00199 ECL 00.05
- VTC accessory channel 1 = BCU II: Z117485/0594 ECL 01.00
- VTC accessory channel 2 = N2-LEVELSONDE 12/1126/850 D325: Z122404/00000 ECL 00.00

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

Prodigy Control Unit: PCU - LNP PRODIGY UNIT Z127349/779
- TCP/IP address   = 192.168.98.2

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99

Magnet System: BZH 657'60'70H04_D325-54-10974 Z115312/MSC10974 ECL H
- Magnet  : BZH 657'600'70H
- Cryostat: D325'54-10974
- Polarity: SN (Bruker)


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 2 of transmitter 2 (AV4 BLABBH500/100 200-600 W144061/000979 at TCP/IP 192.168.99.11)
TRX1 AUX  output -> input 1 of transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/01466 at TCP/IP 192.168.99.10)
TRX2 NORM output -> input 1 of transmitter 2 (AV4 BLABBH500/100 200-600 W144061/000979 at TCP/IP 192.168.99.11)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 1 (AV4 BLABB500 15-600 W144059/000514 at TCP/IP 192.168.99.12)
TRX3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB500 15-600 W144059/000514 at TCP/IP 192.168.99.12:
- amplifier B-500W uses blanking 3

transmitter 2 = AV4 BLABBH500/100 200-600 W144061/000979 at TCP/IP 192.168.99.11:
- amplifier B-500W uses blanking 2
- amplifier 1H-100W uses blanking 1

transmitter 3 = BSMS/2 LOCK TRANSCEIVER 600 Z109890/01466 at TCP/IP 192.168.99.10:
- amplifier 2H-5W uses blanking 9


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX1 -> 2H          -> REC1
Tune-TRX2 -> XBB19F 2HP  -> REC2
Tune-TRX2 -> 13C/79Br    -> REC2
Tune-TRX3 -> 15N         -> REC3

